**Ceiling Speaker T-575**

 

Features:   
Multi-power selection flame-retardant fire-resistant ceiling speaker. Built-in temperature cut-out, T-575 uses 2 frequency division coaxial design, clear and full sound, ideal for your fire sound. Applicable to: shopping malls, supermarkets, hotels, etc.

|  |  |
| --- | --- |
| Model | T-575 |
| Rated Power (100V) | 0.38W, 0.75W, 1.5W, 3W, 6W |
| Rated Power (70V) | 0.19W, 0.38W, 0.75W, 1.5W, 3W |
| Maximum Sensitivity | 100dB |
| Sensitivity | 92dB |
| Impedance | Com / 26KΩ/ 13KΩ/ 6.7KΩ/ |
|  | 3.3KΩ/ 1.7KΩ |
| Frequency Response (-10dB) | 120-18KHz |
| Speaker Unit | 6"×1 1.5"×1 |
| Installation Opening Size | φ207mm |
| Size | 230×126mm |
| Weight | 1.6Kg |